IHE Change Proposal

Tracking information:

|  |  |
| --- | --- |
| IHE Domain | Patient Care Coordination |
| Change Proposal ID: | CP-PCC-xxx |
| Change Proposal Status: | Submitted |
| Date of last update: | 2018-03-09 |
| Person assigned: |  |

Change Proposal Summary information:

|  |  |
| --- | --- |
| WD typeCode for XTHM-WD | |
| Submitter’s Name(s) and e-mail address(es): | Gregorio Canal (gcanal@consorzioarsenal.it) |
| Submission Date: | 2018-03-12 |
| Integration Profile(s) affected: | XTHM-WD |
| Actor(s) affected: | None |
| IHE Technical Framework or Supplement modified: | IHE\_PCC\_Suppl\_XTHM-WD\_Rev1.2\_TI\_2013-10-04 |
| Volume(s) and Section(s) affected: | Update Table in vol 2 section Y.1 |
| Rationale for Change:  LOINC has not yet defined the the OID to be used for the typeCode. At this point PCC should define it and update the supplement.  For more details see [https://groups.google.com/d/msgid/pcctech/50cde85a-d10c-44e1-b13e-3c57b6b36e44%40googlegroups.com](https://groups.google.com/d/msgid/pcctech/50cde85a-d10c-44e1-b13e-3c57b6b36e44%40googlegroups.com?utm_medium=email&utm_source=footer) | |

Editor: Update Table Y.1-2 as follows.

## XTHM Workflow Definition - XDW Workflow Document – Common Attributes

This workflow definition profile is assigned a specific OID that shall be used to assign an identifier to the workflowDefinitionReference element of a Workflow Document that tracks a telemonitoring process.

Table Y.1-1: XTHM-WD Workflow – Workflow Definition Reference

|  |  |
| --- | --- |
| type of Workflow | Workflow Definition Reference |
| Telemonitoring workflow | 1.3.6.1.4.1.19376.1.5.3.1.5.2 |

The XTHM-WD Workflow Definition does not introduce new metadata and all the metadata elements used are the common XDS document metadata specified in ITI TF-3:4.1.5 and in ITI TF-3:5.4.6. In this section only the use of some specific metadata for use of XDW in the XTHM-WD context is specified.

Table Y.1-2: XTHM-WD Workflow – XDS Metadata Attribute

| XDS Metadata Attribute | Definition |
| --- | --- |
| typeCode | For the Workflow Document which tracks the XTHM-WD process the code for the typeCode shall be: (insert code and CodingScheme defined by the PCC)  **~~This code will be assigned by LOINC~~** |
| classCode | For the Workflow Document which tracks the XTHM-WD process the code for the classCode is defined by the XDW profile.  See XDW Supplement Section 5.4.6.1 |
| eventCodeList | **Rule 1:**  An XTHM-WD workflow shall be created with code OPEN and shall remain in this status until it is set to CLOSE.  **Rule 2:**  An XTHM-WD workflow should be set to CLOSE when there is the need to end the telemonitoring workflow for any reason. This is done when the status of the task “CloseTelemonitoringService” is moved to COMPLETED  **Rule 3:**  An XTHM-WD workflow that was set to CLOSE can be reopened and set to OPEN if the patient has a need to use the telemonitoring service again.  See IHE ITI TF-3: 5.4.5.7 for a general description of this attribute. |
| serviceStartTime | Is the time at which work began on the first task for this workflow. |
| serviceStopTime | Is the time at which the status of the overall Workflow is changed from OPEN to CLOSED.  It shall be empty when the workflow is still in OPEN state. |